#---------------
# Undercarriage
#---------------
#
# Format: gear_part = [ posx posy posz
#                       compression_coeff
#                       damping_coeff
#                       max_compression
#                       static_resistance
#                       kinetic_resistance
#                       brakes_resistance ]

#gear_part = [ -0.2 0.0 0.58 50000 10000 0.1 0.9 0.08 0.4 ]	# Main wheel
#gear_part = [ 2.2 0.0 0.56 17355 3500 0.07  0.9 0.08 0.0 ] 	# Nose wheel
#gear_part = [ -5.4 0.0 -0.05 8550 1800 0.07 0.9 0.08 0.0 ] 	# Tail wheel
#gear_part = [ 0.0 -8.75 -0.1 1750 700 0.2 1.8 1.8 0.0 ]    	# Left wing skid
#gear_part = [ 0.0  8.75 -0.1 1750 700 0.2 1.8 1.8 0.0 ]    	# Right wing skid

gear_part {
  name      = Main Wheel
  pos       = [ -0.2 0.0 0.64 ]
  c_comp    = 50000
  c_damp    = 10000
#  max_comp  = 0.1
  max_comp  = 0.5
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.4
}

gear_part {
  name      = Nose Wheel
  pos       = [ 2.2 0.0 0.62 ]
  c_comp    = 17355
  c_damp    = 3500
#  max_comp  = 0.07
  max_comp  = 0.2
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.0
}

gear_part {
  name      = Tail Wheel
  pos       = [ -5.4 0.0 -0.05 ]
  c_comp    = 8550
  c_damp    = 1800
#  max_comp  = 0.07
  max_comp  = 0.2
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.0
}

gear_part {
  name      = Left Wing Skid
  pos       = [ 0.0 -8.75 -0.3 ]
  c_comp    = 1750
  c_damp    = 2000
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 1.0
  r_kinetic = 1.0
  r_brake   = 0.0 
#  load_limit = 10000
#  gfx_node  = wing flex control left inner
}

gear_part {
  name      = Right Wing Skid
  pos       = [ 0.0 8.75 -0.3 ]
  c_comp    = 1750
  c_damp    = 2000
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 1.0
  r_kinetic = 1.0
  r_brake   = 0.0
#  load_limit = 10000
#  gfx_node  = wing flex control right inner
}

gear_part {
  name      = Elevator hardpoint
  pos       = [ -5.4 0.0 -2.0 ]
  c_comp    = 1750
  c_damp    = 700
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0 
}

gear_part {
  name      = Cockpit top hardpoint
  pos       = [ 2.2 0.0 -1.2 ]
  c_comp    = 5000
  c_damp    = 1000
#  max_comp  = 0.2
  max_comp  = 5.0
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0 
}

impact_limit = 30000



