#---------------
# Undercarriage
#---------------

gear_part {
  name      = Main Wheel
  pos       = [ 0.518 0.0 0.6 ]
  c_comp    = 30000
  c_damp    = 7000
#  max_comp  = 0.1
  max_comp  = 0.5
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.4
  retractable = true
  load_limit = 10000
#  gfx_node  = wheel
}

gear_part {
  name      = wheel retract hardpoint
  pos       = [ 1.0 0.0 0.45 ]
  c_comp    = 20000
  c_damp    = 5000
#  max_comp  = 0.2
  max_comp  = 5.0
  r_static  = 1.0
  r_kinetic = 1.0
  r_brake   = 0.0 
}

gear_part {
  name      = Nose
  pos       = [ 2.3 0.0 0.0 ]
  c_comp    = 20000
  c_damp    = 10000
  max_comp  = 0.5
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0
}

gear_part {
  name      = Tail Wheel
  pos       = [ -4.625 0.0 -0.02 ]
  c_comp    = 10000
  c_damp    = 2000
  max_comp  = 0.5
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.0
  steerable = true
  steer_angle = -25.0
}

gear_part {
  name      = Left Wing Skid
  pos       = [ 0.0 -10.0 -0.70 ]
  c_comp    = 1200
  c_damp    = 1000
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.0 
}

gear_part {
  name      = Right Wing Skid
  pos       = [ 0.0 10.0 -0.70 ]
  c_comp    = 1200
  c_damp    = 1000
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.0 
}

gear_part {
  name      = Elevator hardpoint
  pos       = [ -5.4 0.0 -2.0 ]
  c_comp    = 1200
  c_damp    = 700
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0 
}

gear_part {
  name      = Cockpit top hardpoint
  pos       = [ 2.2 0.0 -1.2 ]
  c_comp    = 5000
  c_damp    = 1000
#  max_comp  = 0.2
  max_comp  = 5.0
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0 
}

impact_limit = 30000

