#---------------
# Undercarriage
#---------------
#
# Format: gear_part = [ posx posy posz
#                       compression_coeff
#                       damping_coeff
#                       max_compression
#                       static_resistance
#                       kinetic_resistance
#                       brakes_resistance ]

gear_part {
  name      = Main Wheel
  pos       = [ 0.085 0.0 0.797 ]
  c_comp    = 50000
  c_damp    = 10000
#  max_comp  = 0.1
  max_comp  = 0.5
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.4
  retractable = true
}

gear_part {
  name      = Nose 
  pos       = [ 1.4316 0.0 0.605 ]
  c_comp    = 17355
  c_damp    = 3500
#  max_comp  = 0.07
  max_comp  = 0.2
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0
}

gear_part {
  name      = Tail Wheel
  pos       = [ -4.1118 0.0 0.3534 ]
  c_comp    = 8550
  c_damp    = 1800
#  max_comp  = 0.07
  max_comp  = 0.2
  r_static  = 0.9
  r_kinetic = 0.08
  r_brake   = 0.0
}

gear_part {
  name      = Left Wing Skid
  pos       = [ -0.4239 -7.2332 -0.3097 ]
  c_comp    = 1750
  c_damp    = 2000
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0 
}

gear_part {
  name      = Right Wing Skid
  pos       = [ -0.4239 7.2332 -0.3097 ]
  c_comp    = 1750
  c_damp    = 2000
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0 
}

gear_part {
  name      = Elevator hardpoint
  pos       = [ -4.1374 0.0 -1.1956 ]
  c_comp    = 1750
  c_damp    = 700
#  max_comp  = 0.2
  max_comp  = 2.0
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0 
}

gear_part {
  name      = Cockpit top hardpoint
  pos       = [ 0.7394 0.0 -0.3175 ]
  c_comp    = 5000
  c_damp    = 1000
#  max_comp  = 0.2
  max_comp  = 5.0
  r_static  = 1.8
  r_kinetic = 1.8
  r_brake   = 0.0 
}

impact_limit = 30000

