#--------------------------------------------
# Antares electrical propulsion system setup
# Part of Silent Wings soaring simulator
#--------------------------------------------

aero_coordinate_system = true
reference_position     = [ -2.020 0.0 0.0 ]

# Propeller/engine position
position        = [ 2.50 0.0 1.5 ]

# Propeller pylon drag coefficient and reference area
cd              = 0.15
ref_area        = 1.0

# Max engine power (W), torque (Nm)
power           = 42000.0
torque          = 220.0

# Engine details
engine_rpm_max  = 1700
engine_inertia  = 0.4
engine_friction = 0.1

# Battery capacity (Wh)
capacity        = 9500.0

# Propeller data
prop_diameter   = 2.0
prop_pitch      = 90.0
prop_chord      = 0.20
prop_cd         = 0.008

# Antares one-lever-control parameters:
# 0 = throttle all way back, 1 = full throttle
# Engine will extend/retract around this value, there is a builtin 0.05 hysteresis
pot_extend      = 0.1
# Engine idle position at this value, all above this is linear throttle control.
pot_idle        = 0.35
