#-----------------------
# Control sensitivities
#-----------------------
ailerons_step	   = 0.1
elevator_step	   = 0.1
elevator_trim_step = 0.01
rudder_step	   = 0.1
flaps_step	   = 0.2
airbrakes_step	   = 0.2
wheelbrakes_step   = 0.5
throttle_step	   = 0.05

# Here the Antares flap positions and corresponding flap deflections
#                     -3   -2  -1  0    +1   +2/L
flaps_deflections = [ -3.0 0.0 5.0 10.0 15.0 18.0 ]

#------------------------
# Other control settings
#------------------------

wheelbrakes_on_airbrakes = true

